## Automated ELK Stack Deployment

The files in this repository were used to configure the network depicted below.

![TODO: Update the path with the name of your diagram](Images/diagram\_filename.png)

These files have been tested and used to generate a live ELK deployment on Azure. They can be used to either recreate the entire deployment pictured above. Alternatively, select portions of the playbook file may be used to install only certain pieces of it, such as Filebeat.

- \_TODO: Enter the playbook file.\_

This document contains the following details:

- Description of the Topologu

- Access Policies

- ELK Configuration

- Beats in Use

- Machines Being Monitored

- How to Use the Ansible Build

### Description of the Topology

The main purpose of this network is to expose a load-balanced and monitored instance of DVWA, the D\*mn Vulnerable Web Application.

Load balancing ensures that the application will be highly available, in addition to restricting access to the network.

- \_TODO: What aspect of security do load balancers protect? What is the advantage of a jump box?\_

**\* A jumpbox server serves as a gateway to gain entry into a remote network. Many times the primary mode of access is ssh and without the key access is forbidden.**

**\* A loadbalancer is meant to serve as a specific point of access for a service that is served by multiple machines. This allows high availability models to function properly.**

Integrating an ELK server allows users to easily monitor the vulnerable VMs for changes to the \_\_\_\_\_ and system \_\_\_\_\_.

- \_TODO: What does Filebeat watch for?\_Filebeat is meant to primarily watch for system logs and forward any changes to the Elasticsearch host.

- \_TODO: What does Metricbeat record?\_Metricbeat is used only for gathering metrics and system resources usage for display in Elasticsearch.

The configuration details of each machine may be found below.

\_Note: Use the [Markdown Table Generator](http://www.tablesgenerator.com/markdown\_tables) to add/remove values from the table\_.

| Name | Function | IP Address | Operating System |

|----------|----------|------------|------------------|

| Jump Box | Gateway | 10.0.0.1 | Ubuntu |

| Web1 | Webserver | 10.0.0.4 | Ubuntu |

| Web2 | Webserver | 10.0.0.5 | Ubuntu |

| Elk | ElasticSearch | 10.1.0.4 | Ubuntu |

### Access Policies

The machines on the internal network are not exposed to the public Internet.

Only the jumpbox machine can accept connections from the Internet. Access to this machine is only allowed from the following IP addresses:

- \_TODO: Add whitelisted IP addresses 75.22.119.28

Machines within the network can only be accessed by \_\_\_\_\_.

- \_TODO: Which machine did you allow to access your ELK VM? What was its IP address?\_

Jumpbox PrivateIP: 10.1.0.4 PublicIP: 20.102.107.57

A summary of the access policies in place can be found in the table below.

| Name | Publicly Accessible | Allowed IP Addresses |

|----------|---------------------|----------------------|

| Jump Box | SSH – 22 Yes | 75.22.119.28 |

| Web 1, 2 | No | Web LB |

| Elk | No | |

### Elk Configuration

Ansible was used to automate configuration of the ELK machine. No configuration was performed manually, which is advantageous because...

- \_TODO: What is the main advantage of automating configuration with Ansible?\_


The playbook implements the following tasks: It allows changes to be made within any of the VM’s associated with it.

- \_TODO: In 3-5 bullets, explain the steps of the ELK installation play. E.g., install Docker; download image; etc.\_ Install Docker.io; download image; install python3-pip; download and configure an elk-docker container; launch the elk-docker container.

- ...

- ...

The following screenshot displays the result of running `docker ps` after successfully configuring the ELK instance.



![TODO: Update the path with the name of your screenshot of docker ps output]( "C:\Users\jessi\OneDrive\Pictures\project13snippet.PNG"

### Target Machines & Beats

This ELK server is configured to monitor the following machines:

- \_TODO: List the IP addresses of the machines you are monitoring\_10.0.0.4, 10.0.0.5 and 10.0.0.6

We have installed the following Beats on these machines:

- \_TODO: Specify which Beats you successfully installed: Filebeat and Metricbeat.

These Beats allow us to collect the following information from each machine:

- \_TODO: In 1-2 sentences, explain what kind of data each beat collects, and provide 1 example of what you expect to see. E.g., `Winlogbeat` collects Windows logs, which we use to track user logon events, etc.

**Filebeat monitors the log files or locations that you specify, collects log events, and forwards them either to Elasticsearch or Logstash for indexing.**

**Metricbeat collects metric data from your target servers, this could be operating system metrics such as CPU or memory or data related to services running on the server. It can also be used to monitor other beats and ELK stack itself.**

### Using the Playbook

In order to use the playbook, you will need to have an Ansible control node already configured. Assuming you have such a control node provisioned:

SSH into the control node and follow the steps below:

- Copy the ansible config file to run playbook.

- Update the ansible host file to include...

- Run the playbook, and navigate to Jumpbox to check that the installation worked as expected.

\_TODO: Answer the following questions to fill in the blanks:\_

- \_Which file is the playbook? Where do you copy it? **Elk-playbook.yml**

- \_Which file do you update to make Ansible run the playbook on a specific machine? **Update the hosts file or the ansible.cfg.**

How do I specify which machine to install the ELK server on versus which to install Filebeat on?\_**By using the IP of the server running.**

- \_Which URL do you navigate to in order to check that the ELK server is running? **http://thatdaysipaddress:5601/app/kibana**

\_As a \*\*Bonus\*\*, provide the specific commands the user will need to run to download the playbook, update the files, etc.\_